A signal has a bandwidth of 6kHz. It is sampled, logarithmically compressed and encoded into a PCM format using 8bits per sample. The PCM data is transmitted through an AWGN channel via M-PSK. Determine the minimum bandwidth required for the transmission when

1. M=4;
2. M=8;
3. M=16.